**HAMERSLEY ROAD - LOCALISED REALIGNMENT: SCOPE OF WORKS**

In order to facilitate the safe turning circle of Double Road Trains, the existing Hamersley Road is required to be widened at four (4) localised areas.

# Scope of Works

* Survey to set out extent of works
* Clearing, Grubbing and Topsoil Strip to design extent
* Foundation Preparation
* Sheeting of the widened area (if required based on road condition)
* Installation of cut off drains to manage surface water flow

The following plant and equipment will be associated with the widening works:

* Grader
* Loader
* Smooth Drum Roller
* Water Truck

The above works will be carried out under FMG Supervision.

# Program of Works

Works are programmed to be undertaken from August 2020 pending Heritage and Environmental approval and the works will take approximately 3 weeks.